<< Previous | Next >>

> ADD A,n Add Without Carry Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> C6 n | ADD A,n | 4 (2,2) | A = A + n

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | V | · | · | · |  |  |

> #### Description

> A is summed with the 8-bit constant n. The result is stored in A.

> The Rabbit 4000 assembler views "ADD A,n" and "ADD n" as equivalent instructions. In the latter case, A is used even though it is not explicitly stated.

<< Previous | Next >>