<< Previous | Next >>

> AND IX,DE
> AND IY,DE Bitwise AND Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD DC | AND IX,DE | 4 (2,2) | IX = IX & DE
> FD DC | AND IY,DE | 4 (2,2) | IY = IY & DE

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · |  |  |  |

> #### Description

> Performs a bitwise AND operation between IX or IY and DE. The result is stored in IX or IY.

<< Previous | Next >>