<< Previous | Next >>

> LD pd,JKHL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> -- | LD pd,JKHL | 4 (2,2) | pd = JKHL
> FD 8D | LD PW,JKHL | 4 (2,2) | PW = JKHL
> FD 9D | LD PX,JKHL | 4 (2,2) | PX = JKHL
> FD AD | LD PY,JKHL | 4 (2,2) | PY = JKHL
> FD BD | LD PZ,JKHL | 4 (2,2) | PZ = JKHL

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads pd (any of the 32-bit registers PW, PX, PY or PZ) with JKHL.

<< Previous | Next >>