<< Previous | Next >>

> ADC A,n Add With Carry Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> CE n | ADC A,n | 4 (2,2) | A = A + n + CF

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | V | · | · | · |  |  |

> #### Description

> The 8-bit constant n is summed with the C flag and A. The sum is stored in A.

> The Rabbit 4000 assembler views "ADC A,n" and "ADC n" as equivalent instructions. In the latter case, A is used even though it is not explicitly stated.

<< Previous | Next >>