<< Previous | Next >>

> LD IY,(mn) Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> FD 2A n m | LD IY,(mn) | 13 (2,2,2,2,1,2,2) | IYlow = (mn) IYhigh = (mn + 1)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  | · |

> #### Description

> Loads IY with the data whose address is the 16-bit constant mn.

<< Previous | Next >>