<< Previous | Next >>

> POP IP
> POP IX
> POP IY Stack Operation Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> ED 7E | POP IP | 7 (2,2,1,2) | IP = (SP) SP = SP + 1
> DD E1 | POP IX | 9 (2,2,1,2,2) | IXlow = (SP) IXhigh = (SP + 1) SP = SP + 2
> FD E1 | POP IY | 9 (2,2,1,2,2) | IYlow = (SP) IYhigh = (SP + 1) SP = SP + 2

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Pops IP, IX or IY from the stack.

> POP IP is a chained-atomic instruction.

<< Previous | Next >>