<< Previous | Next >>

> LD SP,HL
> LD SP,IX
> LD SP,IY Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> F9 | LD SP,HL | 2 | SP = HL
> DD F9 | LD SP,IX | 4 (2,2) | SP = IX
> FD F9 | LD SP,IY | 4 (2,2) | SP = IY

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads SP with:

> - HL, or
> - IX, or
> - IY

> These are chained-atomic instructions, meaning that an interrupt cannot take place between one of these instructions and the instruction following it.

<< Previous | Next >>