<< Previous | Next >>

> LD XPC,A Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> ED 67 | LD XPC,A | 4 (2,2) | XPC = A

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads XPC with A. This is a chained-atomic instruction, meaning that an interrupt cannot take place between this instruction and the instruction following it.

<< Previous | Next >>