<< Previous | Next >>

> LD A,(IX+A)
> LD A,(IY+A) Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD 06 | LD A,(IX+A) | 8 (2,2,2,2) | A = (IX + A)
> FD 06 | LD A,(IY+A) | 8 (2,2,2,2) | A = (IY + A)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  | · |

> #### Description

> Loads A with the data whose address is

> - the sum of IX and A, or
> - the sum of IY and A.

> A is considered an 8-bit unsigned offset. These instructions are useful for accessing 256-byte lookup tables.

<< Previous | Next >>