<< Previous | Next >>

> OR (HL) Bitwise OR Rabbit 2000/30000/3000A Instruction

> Opcode | Instruction | Clocks | Operation
> B6 | OR (HL) | 5 (2,1,2) | A = A | (HL)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · | · |  | · |

> #### Description

> Performs a bitwise OR operation between A and the data whose address is in HL.The result is stored in A.

> #### Example

> If the byte in A is 0100 1100 and the byte in the memory location pointed to by HL is 1110 0101, the operation:

>     OR (HL)

> would result in A containing 1110 1101.

<< Previous | Next >>