<< Previous | Next >>

> RLA Rotate Left A Through Carry Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 17 | RLA | 2 | {CF,A} = {A,CF}

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | · | · | · |  |  |

> #### Description

> Rotates to the left with the C flag the contents of A. Each bit in the register moves to the next highest-order bit position (bit 0 moves to bit 1, etc.) while the C flag moves to bit 0 and bit 7 moves to the C flag. See Figure 3 for an illustration.

<< Previous | Next >>