<< Previous | Next >>

> NEG BCDE
> NEG JKHL Negate Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD 4D | NEG BCDE | 4 (2,2) | BCDE = 0 - BCDE
> FD 4D | NEG JKHL | 4 (2,2) | JKHL = 0 - JKHL

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | V | · | · | · |  |  |

> #### Description

> Subtracts BCDE or JKHL from zero and stores the result in BCDE or JKHL.

<< Previous | Next >>