<< Previous | Next >>

> LD HL,(SP+n) Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> C4 n | LD HL,(SP+n) | 9 (2,2,1,2,2) | L = (SP + n) H = (SP + n + 1)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> Loads HL with the data whose address is the sum of SP and the 8-bit unsigned constant n.

<< Previous | Next >>