<< Previous | Next >>

> XOR HL,DE
> XOR JKHL,BCDE Exclusive OR Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 54 | XOR HL,DE | 4 (2,2) | HL = HL ^ DE
> ED EE | XOR JKHL,BCDE | 4 (2,2) | JKHL = JKHL ^ BCDE

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · | · |  |  |

> #### Description

> - `XOR HL,DE`: This instruction performs an exclusive OR operation between the word in HL and the word in DE. The result is stored in HL.

> - `XOR JKHL,BCDE`: This instruction performs an exclusive OR operation between the 32-bit value in JKHL and the 32-bit value in BCDE. The result is stored in JKHL.

<< Previous | Next >>