<< Previous | Next >>

> LDF (lmn),A
> LDF (lmn),HL Load Far Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 8A n m l | LDF (lmn),A | 12 (2,2,2,2,1,3) | (lmn) = A
> 82 n m l | LDF (lmn),HL | 15 (2,2,2,2,1,3,3) | (lmn) = L (lmn + 1) = H

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose physical address is the 24-bit constant lmn with:

> - A, or

> - HL

<< Previous | Next >>