<< Previous | Next >>

> LD JKHL,(SP+n) Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> FD EE n | LD JKHL,(SP+n) | 15 (2,2,2,1,2,2,2,2) | L = (SP + n) H = (SP + n + 1) K = (SP + n + 2) J = (SP + n + 3)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> Loads JKHL with the data whose address is the sum of SP and the 8-bit unsigned constant n.

<< Previous | Next >>