<< Previous | Next >>

> LD (IX+d),BCDE
> LD (IX+d),JKHL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD CF d | LD (IX+d),BCDE | 19 (2,2,2,1,3,3,3,3) | (IX + d) = E (IX + d + 1) = D (IX + d + 2) = C (IX + d + 3) = B
> FD CF d | LD (IX+d),JKHL | 19 (2,2,2,1,3,3,3,3) | (IX + d) = L (IX + d + 1) = H (IX + d + 2) = JKlow (IX + d +3) = JKhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is the sum of IX and the 8-bit signed displacement d with

> - BCDE, or
> - JKHL

<< Previous | Next >>