<< Previous | Next >>

> RLC 8,BCDE
> RLC 8,JKHL Rotate Left Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD 4F | RLC 8,BCDE | 4 (2,2) | BCDE = {CDE,B}
> FD 4F | RLC 8,JKHL | 4 (2,2) | JKHL = {KHL,J}

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Rotates BCDE or JKHL to the left. Each byte moves to the next highest-order byte position, with the highest-order byte moving to the lowest-order byte. See the figure below.

> Figure 8: Bit logic of "RLC 8,BCDE" instruction

<< Previous | Next >>