<< Previous | Next >>

> ADD A,(HL) Add Without Carry Rabbit 2000/3000/3000A Instruction

> Opcode | Instruction | Clocks | Operation
> 86 | ADD A,(HL) | 5 (2,1,2) | A = A + (HL)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | V | · | · | · |  | · |

> #### Description

> A is summed with the data whose address is in HL. The result is stored in A.

> The opcode for this instruction is different than the same instruction in the Rabbit 4000.

<< Previous | Next >>