<< Previous | Next >>

> LDF A,(lmn)
> LDF HL,(lmn) Load Far Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 9A n m l | LDF A,(lmn) | 11 (2,2,2,2,1,2) | A = (lmn)
> 92 n m l | LDF HL,(lmn) | 13 (2,2,2,2,1,2,2) | L = (lmn) H = (lmn + 1)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> Loads A or HL with the data whose physical address is the 24-bit constant lmn.

<< Previous | Next >>