<< Previous | Next >>

> RRC 8,BCDE
> RRC 8,JKHL Rotate Right Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD 5F | RRC 8,BCDE | 4 (2,2) | BCDE = {E, BCD}
> FD 5F | RRC 8,JKHL | 4 (2,2) | JKHL = {L, JKH}

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Rotates BCDE or JKHL to the right. Each byte in the register moves to the next lowest-order byte position. E.g., the byte in B is loaded into C; the byte that was in C is loaded into D; the byte that was in D is loaded into E; and the byte that was in E is loaded into B.

> Figure 17: The bit logic of the "RRC 8,BCDE" instruction

<< Previous | Next >>