<< Previous | Next >>

> OR IX,DE
> OR IY,DE Bitwise OR Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD EC | OR IX,DE | 4 (2,2) | IX = IX | DE
> FD EC | OR IY,DE | 4 (2,2) | IY = IY | DE

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · |  |  |  |

> #### Description

> Performs a bitwise OR operation between DE and

> - IX, or
> - IY

> The result is stored in IX or IY.

<< Previous | Next >>