<< Previous | Next >>

> LD (SP+n),BCDE
> LD (SP+n),JKHL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD EF n | LD (SP+n),BCDE | 19 (2,2,2,1,3,3,3,3) | (SP + n) = E (SP + n + 1) = D (SP + n + 2) = C (SP + n + 3) = B
> FD EF n | LD (SP+n),JKHL | 19 (2,2,2,1,3,3,3,3) | (SP + n) = L (SP + n + 1) = H (SP + n + 2) = JKlow (SP + n + 3) = JKhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is the sum of SP and the 8-bit unsigned constant n with BCDE or JKHL.

<< Previous | Next >>