<< Previous | Next >>

> LD (IY+d),BCDE
> LD (IY+d),JKHL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD DF d | LD (IY+d),BCDE | 19 (2,2,2,1,3,3,3,3) | (IY + d) = E (IY + d + 1) = D (IY + d + 2) = C (IY + d + 3) = B
> FD DF d | LD (IY+d),JKHL | 19 (2,2,2,1,3,3,3,3) | (IY + d) = L (IY + d + 1) = H (IY + d + 2) = JKlow (IY + d + 3) = JKhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is the sum of IY and the 8-bit signed displacement d with

> - BCDE, or
> - JKHL

<< Previous | Next >>