<< Previous | Next >>

> LD (mn),BCDE
> LD (mn),JKHL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 83 n m | LD (mn),BCDE | 19 (2,2,2,1,3,3,3,3) | (mn) = E (mn + 1) = D (mn + 2) = C (mn + 3) = B
> 84 n m | LD (mn),JKHL | 19 (2,2,2,1,3,3,3,3) | (mn) = L (mn + 1) = H (mn + 2) = JKlow (mn + 3) = JKhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is mn with BCDE or JKHL.

<< Previous | Next >>