<< Previous | Next >>

> RRA Rotate Right A Through Carry Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 1F | RRA | 2 | {A,CF} = {CF,A}

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | · | · | · |  |  |

> #### Description

> Rotates to the right with the C flag the data in A. Bit 0 moves to the C flag, bits 1 through 7 move to the next lowest-order bit position, and the C flag moves to bit 7. See Figure 12 for an illustration.

<< Previous | Next >>