<< Previous | Next >>

> LD LXPC,HL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 97 | LD LXPC,HL | 2 | LXPClow = L LXPChigh = H

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the 12-bit LXPC with HL. The most significant 4 bits of HL are ignored. This is a chained-atomic instruction, meaning that an interrupt cannot take place between this instruction and the instruction following it.

<< Previous | Next >>