<< Previous | Next >>

> AND r Bitwise AND Rabbit 2000/3000/3000A Instruction

> Opcode | Instruction | Clocks | Operation
> ---- | AND r | 2 | A = A & r
> A7 | AND A | 2 | A = A & A
> A0 | AND B | 2 | A = A & B
> A1 | AND C | 2 | A = A & C
> A2 | AND D | 2 | A = A & D
> A3 | AND E | 2 | A = A & E
> A4 | AND H | 2 | A = A & H
> A5 | AND L | 2 | A = A & L

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · | · |  |  |

> #### Description

> Performs a bitwise AND operation between A and r (any of the registers A, B, C, D, E, H, or L). The result is stored in A.

> The opcodes for these instructions are different than the same instructions in the Rabbit 4000.

<< Previous | Next >>