<< Previous | Next >>

> ADC HL,ss Add With Carry Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> ---- | ADC HL,ss | 4 (2,2) | HL = HL + ss + CF
> ED 4A | ADC HL,BC | 4 (2,2) | HL = HL + BC + CF
> ED 5A | ADC HL,DE | 4 (2,2) | HL = HL + DE + CF
> ED 6A | ADC HL,HL | 4 (2,2) | HL = HL + HL + CF
> ED 7A | ADC HL,SP | 4 (2,2) | HL = HL + SP + CF

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | V | · | · | · |  |  |

> #### Description

> HL is summed with the C flag and with ss (any of BC, DE, HL, or SP). The result is stored in HL.

<< Previous | Next >>