<< Previous | Next >>

> LD A,XPC Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> ED 77 | LD A,XPC | 4 (2,2) | A = XPC

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> Loads A with XPC.

> This is a chained-atomic instruction, meaning that an interrupt cannot take place between this instruction and the instruction following it.

<< Previous | Next >>