<< Previous | Next >>

> LD BCDE,(HL) Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD 1A | LD BCDE,(HL) | 14 (2,2,2,2,2,2,2) | E = (HL) D = (HL + 1) C = (HL + 2) B = (HL + 3)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> The 32-bit register BCDE is loaded with the 4 bytes of data whose address starts at HL.

<< Previous | Next >>