<< Previous | Next >>

> LD (HL),JKHL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> FD 1B | LD (HL),JKHL | 18 (2,2,2,3,3,3,3) | (HL) = L (HL + 1) = H (HL + 2) = JKlow (HL + 3) = JKhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is in HL with JKHL.

<< Previous | Next >>