<< Previous | Next >>

> LD JKHL,(IX+d)
> LD JKHL,(IY+d) Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> FD CE d | LD JKHL,(IX+d) | 15(2,2,2,1,2,2,2,2) | JKHL= (IX + d)
> FD DE d | LD JKHL,(IY+d) | 15(2,2,2,1,2,2,2,2) | JKHL= (IY + d)

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> Loads JKHL with the data whose address is

> - the sum of IX and the 8-bit signed displacement d, or

> - the sum of IY and the 8-bit signed displacement d

<< Previous | Next >>