<< Previous | Next >>

> LD (HL+d),HL Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD F4 d | LD (HL+d),HL | 13 (2,2,2,1,3,3) | (HL + d) = L (HL + d + 1) = H

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  | ·

> #### Description

> Loads the memory location whose address is the sum of HL and the 8-bit signed displacement d with HL.

<< Previous | Next >>