<< Previous | Next >>

> OR r Bitwise OR Rabbit 2000/30000/3000A Instruction

> Opcode | Instruction | Clocks | Operation
> ---- | OR r | 2 | A = A | r
> B0 | OR B | 2 | A = A | B
> B1 | OR C | 2 | A = A | C
> B2 | OR D | 2 | A = A | D
> B3 | OR E | 2 | A = A | E
> B4 | OR H | 2 | A = A | H
> B5 | OR L | 2 | A = A | L

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · | · |  |  |

> #### Description

> Performs a bitwise OR operation between A and r (any of the 8-bit registers B, C, D, E, H, or L). The result is stored in A.

> The opcodes for these instructions are different than the same instructions in the Rabbit 4000.

<< Previous | Next >>