<< Previous | Next >>

> JP (HL)
> JP (IX)
> JP (IY)
> JP mn Jump Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> E9 | JP (HL) | 4 (2,2) | PC = HL
> DD E9 | JP (IX) | 6 (2,2,2) | PC = IX
> FD E9 | JP (IY) | 6 (2,2,2) | PC = IY
> C3 n m | JP mn | 7 (2,2,2,1) | PC = mn

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> PC is loaded with HL, IX, IY or the 16-bit constant mn. The Dynamic C assembler recognizes labels as well.

> #### See Also: SJP label

<< Previous | Next >>