<< Previous | Next >>

> LD (pd+d),HL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> -- | LD (pd+d),HL | 11 (2,2,1,3,3) | (pd + d) = L (pd + d + 1) = H
> 86 d | LD (PW+d),HL | 11 (2,2,1,3,3) | (PW + d) = L (PW + d + 1) = H
> 96 d | LD (PX+d),HL | 11 (2,2,1,3,3) | (PX + d) = L (PX + d + 1) = H
> A6 d | LD (PY+d),HL | 11 (2,2,1,3,3) | (PY + d) = L (PY + d + 1) = H
> B6 d | LD (PZ+d),HL | 11 (2,2,1,3,3) | (PZ + d) = L (PZ + d + 1) = H

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is computed as the sum of pd and the 8-bit signed displacement d with HL.

> The address is treated either as a logical address that will be passed through the MMU for translation into a physical address or as a physical address that does not need MMU translation.

> If pd is 0xFFFFxxxx, i.e., the upper 16 bits are all ones, it represents a logical address. This is called a "long logical" address. Otherwise, it is a physical address with the low 20 bits or 24 bits being significant (depending on the memory available).

<< Previous | Next >>