<< Previous | Next >>

> RLCA Rotate Left A Affect Carry Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 07 | RLCA | 2 | A = {A[6,0],A[7]} CF = A[7]

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | · | · | · |  |  |

> #### Description

> Rotates A to the left. Each bit in the register moves to the next highest-order bit position (bit 0 moves to bit 1, etc.) while bit 7 moves to both bit 0 and the C flag. See Figure 7 for an illustration.

<< Previous | Next >>