<< Previous | Next >>

> LDF (lmn),BCDE
> LDF (lmn),JKHL Load Far Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD 0B n m l | LDF (lmn),BCDE | 23 (2,2,2,2,2,1,3,3,3,3) | (lmn) = E (lmn + 1) = D (lmn + 2) = C (lmn + 3) = B
> FD 0B n m l | LDF (lmn),JKHL | 23 (2,2,2,2,2,1,3,3,3,3) | (lmn) = L (lmn + 1) = H (lmn + 2) = JKlow (lmn + 3) = JKhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose physical address is the 24-bit constant lmn with:

> - BCDE, or

> - JKHL

<< Previous | Next >>