<< Previous | Next >>

> LD (SP+n),HL
> LD (SP+n),IX
> LD (SP+n),IY Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> D4 n | LD (SP+n),HL | 11 (2,2,1,3,3) | (SP + n) = L (SP + n + 1) = H
> DD D4 n | LD (SP+n),IX | 13 (2,2,2,1,3,3) | (SP + n) = IXlow (SP + n + 1) = IXhigh
> FD D4 n | LP (SP+n),IY | 13 (2,2,2,1,3,3) | (SP + n) = IYlow (SP + n + 1) = IYhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is the sum of SP and the 8-bit unsigned constant n with HL, IX or IY.

<< Previous | Next >>