<< Previous | Next >>

> LD (SP+HL),BCDE
> LD (SP+HL),JKHL Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD FF | LD (SP+HL),BCDE | 18 (2,2,2,3,3,3,3) | (SP+HL) = E; (SP+HL+1) = D (SP+HL+2) = C; (SP+HL+3) = B
> FD FF | LD (SP+HL),JKHL | 18 (2,2,2,3,3,3,3) | (SP+HL) = L; (SP+HL+1) = H (SP+HL+2) = JKlow (SP+HL+3) = JKhigh

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the memory location whose address is the sum of SP and HL with BCDE or JKHL.

<< Previous | Next >>