<< Previous | Next >>

> LJP x,mn Long Jump Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> C7 n m x | LJP x,mn | 10 (2,2,2,2,2) | XPC = x PC = mn

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> This instruction is similar to the "JP mn" instruction in that it transfers program execution to the memory location specified by the 16-bit constant, mn. LJP is special in that it allows a jump to be made to a computed address in XMEM. Note that the value of XPC and consequently the address space defined by the XPC is dynamically changed with the LJP instructions.

> This instruction recognizes labels when used in the Dynamic C assembler.

> #### See Also: SJP label

<< Previous | Next >>