<< Previous | Next >>

> LD IX,HL
> LD IX,mn
> LD IY,HL
> LD IY,mn Load Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DD 7D | LD IX,HL | 4 (2,2) | IX = HL
> DD 21 n m | LD IX,mn | 8 (2,2,2,2) | IX = mn
> FD 7D | LD IY,HL | 4 (2,2) | IY = HL
> FD 21 n m | LD IY,mn | 8 (2,2,2,2) | IY = mn

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads IX or IY with HL or the 16-bit constant mn.

<< Previous | Next >>