<< Previous | Next >>

> POP SU Stack Operation Rabbit 3000A/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> ED 6E | POP SU | 9 (2,2,2,3) | SU = (SP) SP = SP + 1

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Loads the System/User Mode Register SU with the data at the memory location in SP, then increments the data in SP.

> This is a chained-atomic instruction, meaning that an interrupt cannot take place between this instruction and the instruction following it.

<< Previous | Next >>