<< Previous | Next >>

> INC (HL)
> INC (IX+d)
> INC (IY+d) Increment Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 34 | INC (HL) | 8 (2,1,2,3) | (HL) = (HL) + 1
> DD 34 d | INC (IX+d) | 12 (2,2,2,1,2,3) | (IX+d) = (IX+d) + 1
> FD 34 d | INC (IY+d) | 12 (2,2,2,1,2,3) | (IY+d) = (IY+d) + 1

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | V | - | · |  |  | · | ·

> #### Description

> Increments the byte whose address is:

> - HL, or
> - the sum of IX and the 8-bit signed displacement d, or
> - the sum of IY and the 8-bit signed displacement value d

<< Previous | Next >>