<< Previous | Next >>

> LD BCDE,ps Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> -- | LD BCDE,ps | 4 (2,2) | BCDE = ps
> DD CD | LD BCDE,PW | 4 (2,2) | BCDE = PW
> DD DD | LD BCDE,PX | 4 (2,2) | BCDE = PX
> DD ED | LD BCDE,PY | 4 (2,2) | BCDE = PY
> DD FD | LD BCDE,PZ | 4 (2,2) | BCDE = PZ

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> The 32-bit register BCDE is loaded with ps (any of the 32-bit registers PW, PX, PY or PZ).

<< Previous | Next >>