<< Previous | Next >>

> LD HL,LXPC Load Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 9F | LD HL,LXPC | 2 | HL = LXPC

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  | · |  |  |

> #### Description

> Loads HL with the extended 12-bit XPC (LXPC). This is a chained-atomic instruction, meaning that an interrupt cannot take place between this instruction and the instruction following it.

<< Previous | Next >>