<< Previous | Index | Next >>

> ## Appendix B. Plastic Enclosure

> The plastic enclosure provides a secure way to enclose your RabbitLink board. The enclosure itself may be mounted on any flat surface.

> Appendix B describes how to mount the RabbitLink board inside the plastic enclosure, how to install the optional light pipes, and provides details on mounting the assembly.

> ### B.1 Assembly

> 1. Attach the RabbitLink board to the plastic enclosure base.

>    Position the RabbitLink board over the plastic enclosure base as shown below in Figure B.1-1. Attach the board to the base using the two 4-40 × ¼ screws supplied.

> Figure B.1-1 Attach RabbitLink Board to Plastic Enclosure Base

> 1. Install light pipes (optional).

>    Light pipes are included in the tool kit so you can see the LEDs on the RabbitLink board once the enclosure is assembled.

> Figure B.1-2 Install Light Pipes in Enclosure Top

> With the enclosure top positioned as shown in Figure B.1-2, insert three light pipes into the slots identified in Figure B.1-2. Position the light pipes snugly against the enclosure top since there is little clearance between the light pipes and the LEDs on the RabbitLink board. The light pipes snap in place. Verify that the light pipes are aligned over the LEDs, then apply a drop of cyanoacrylate or contact cement to the inside of the enclosure around each light pipe to hold it in place.

> NOTE | Once the glue is applied, it will not be possible to change the alignment of the light pipes without damaging the plastic enclosure.

> 1. Attach the enclosure top to the base.

>    Position the enclosure top over the plastic enclosure base as shown below in Figure B.1-3. Attach the enclosure top to the base using the two 4-40 × ½ screws supplied. If you installed the light pipes, be sure they are aligned over the LEDs as shown.

> Figure B.1-3 Attach Enclosure Top

> 1. Mount plastic enclosure (optional).

>    Use four #10 screws to attach the assembled plastic enclosure to the surface on which it will be mounted. This step applies to production versions of RabbitLink boards once development has been completed.

> ### B.2 Dimensions

> Figure B.2-1 shows the dimensions for the plastic enclosure.

> Figure B.2-1 Plastic Enclosure Dimensions

> When fully assembled with the RabbitLink installed, the total height of the plastic enclosure will be 1.1" (28 mm).

<< Previous | Index | Next >>
Z-World, Inc. www.zworld.com Phone: 1.530.757.3737 Fax: 1.530.757.3792 | Rabbit Semiconductor www.rabbitsemiconductor.com Phone: 1.530.757.8400 Fax: 1.530.757.8402