Wildcat (BL2000) User's Manual

> A

> - B - C - D - E - F - G - H - I - J - K - L - M - N - O - P - Q - R - S - T - U - V - W - X - Y - Z

> ## Index

> ### A

>   A/D converter
>     buffered inputs 1
>   A/D converter inputs 1
>   analog I/O
>     reference voltages 1
>   analog inputs
>     use as digital inputs 1
>   analog outputs 1

> ### B

>   battery
>     connections 1
>     life 1
>     replacing the backup battery 1

> ### C

>   chip select circuit 1
>   conformal coating 1
>   connections
>     battery 1
>     Ethernet cable 1

> ### D

>   D/A converter outputs 1
>   Demonstration Board 1
>     hookup instructions 1
>       analog sample programs 1
>       digital sample programs 1
>     wire assembly 1
>   digital inputs 1
>     configured pull-up or pull-down 1
>     dual-purpose A/D converter inputs as digital inputs 1
>     switching threshold 1
>   digital outputs 1
>     +K 1
>     pulled up or pulled down 1
>     sinking 1
>     sourcing 1
>   dimensions
>     BL2000 board 1
>     plastic enclosure 1
>   Dynamic C Premier 1, 2
>     basic instructions 1
>     changing programming baud rate in BIOS 1
>     debugging features 1
>     installation 1
>     programming in flash vs. RAM 1
>     starting 1

> ### E

>   Ethernet cables 1
>   Ethernet connections 1
>     steps 1
>   Ethernet port 1
>     ground lug 1
>     handling EMI and noise 1
>     pinout 1
>   external interrupts 1
>     components 1
>     workaround 1

> ### F

>   features 1

> ### H

>   headers
>     JP1 1

> ### I

>   installation
>     plastic enclosure
>       BL2000 1
>       light pipes 1
>       top 1
>   IP addresses 1, 2, 3
>     how to set 1
>     how to set PC IP address 1

> ### J

>   jumper configurations 1, 2
>     J9(12) 1
>     J9(12) is GND 1
>     J9(12) is Vcc 1
>     JP1 (RS-485 bias and termination resistors) 1, 2
>     JP2 (flash memory bank select) 1, 2
>     JP3 (D/A converter power supply) 1, 2
>     JP4 (flash memory size)
>     1, 2
>     JP5 (SRAM size) 1, 2
>     JP6 (digital input pull-up/pull-down resistors) 1, 2
>     jumper locations 1

> ### K

>   K 1

> ### M

>   memory 1
>     flash memory configurations
>     1
>     SRAM configuration for different sizes 1
>   models 1
>     BL2000 1
>     BL2010 1
>     BL2020 1
>     BL2030 1

> ### P

>   pin configurations
>     programming port 1
>   pinout
>     BL2000 headers 1
>     Ethernet port 1
>     programming port 1
>   plastic enclosure 1, 2
>     attach BL2000 to base 1
>     dimensions 1
>   power management 1
>   power supplies 1
>     backup battery circuit 1
>     battery backup 1
>     battery life 1
>     chip select circuit 1
>     switching voltage regulator 1
>     VRAM switch 1
>   power supply 1
>     connections 1, 2
>   Program Mode 1
>   programming
>     flash vs. RAM 1
>     programming cable 1
>     programming port 1
>   programming cable 1
>     connections 1
>     DIAG connector 1
>   programming port
>     pin configurations 1
>     pinout 1
>     used as diagnostic port 1

> ### R

>   Rabbit 2000
>     parallel ports 1
>   relay outputs 1
>     operation in parallel with diigital output OUT0 1
>   reset 1
>     hardware 1
>     reset generator 1
>   RS-232 1
>   RS-485 1
>   RS-485 network 1
>     termination and bias resistors
>     1
>   Run Mode 1
>   running TCP/IP sample programs 1

> ### S

>   sample programs 1
>     A/D converter inputs
>       AD_CALIB.C 1
>       AD1.C 1
>       AD2.C 1
>       AD3.C 1
>       AD4.C 1
>       BOARD_ID.C 1
>       COUNTLEDS.C 1
>       D/A converter outputs
>         DACAL.C 1
>         DAOUT1.C 1
>         DAOUT2.C 1
>       digital I/O
>         ANADIGIN.C 1
>         DIGIN.C 1
>         DIGOUT.C 1
>         LED.C 1
>         PWM.C 1
>         RELAY.C 1
>       how to set IP address 1
>       LEDS_4.C 1
>       PONG.C 1
>       running TCP/IP sample programs 1
>       serial communication
>         MASTER.C 1
>         PUTS.C 1
>         RELAYCHR.C 1
>         SLAVE.C 1
>       TCP/IP 1
>         PINGME.C 1
>         SMTP.C 1
>         SSI.C 1
>         TELNET.C 1
>     serial communication 1
>       programming port 1
>       RS-232 description 1
>       RS-485 description 1
>       RS-485 network 1
>       RS-485 termination and bias resistors 1
>     serial ports
>       Ethernet port 1
>     setup 1
>       attach BL2000 to enclosure base 1
>       power supply connections 1
>       programming cable connections 1
>     software 1
>       A/D converter inputs
>         _anaIn 1
>         anaIn 1
>         anaInCalib 1
>         anaInEERd 1
>         anaInEEWr 1
>         anaInVolts 1
>         board initialization 1
>           brdInit 1
>         D/A converter outputs
>           anaOut 1
>           anaOutCalib 1
>           anaOutEERd 1
>           anaOutEEWr 1
>           anaOutVolts 1
>         digital I/O
>           digIn 1
>           digOut 1
>         LED outputs
>           ledOut 1
>         libraries 1
>           ARP.LIB 1
>           BL2000 1
>           BL20xx.LIB 1
>           BOOTP.LIB 1
>           BSDNAME.LIB 1
>           DCRTCP.LIB 1
>           DNS.LIB 32
>           FTP_CLIENT.LIB 1
>           FTP_SERVER.LIB 1
>           HTTP.LIB 1
>           ICMP.LIB 1
>           IP.LIB 32
>           MD5.LIB 32
>           NET.LIB 32
>           PACKET.LIB 36
>           PKTDRV.LIB 1
>           POP3.LIB 1
>           REALTEK.LIB 32
>           RS232.LIB 1
>           SMTP.LIB 1
>           TCP/IP 1
>           TCP.LIB 32
>           UDP.LIB 32
>           VSERIAL.LIB 1
>           ZSERVER.LIB 32
>         relay output
>           relayOut 1
>         sample programs 1
>           BOARD_ID.C 1
>           COUNTLEDS.C 1
>           LEDS_4.C 1
>           PONG.C 1
>         serial communication
>           flow control 1
>           ser485Rx 1
>           ser485Tx 1
>           serCflowcontrolOff 1
>           serCflowcontrolOn 1
>       specifications
>         dimensions (BL2000) 1
>         dimensions (plastic enclosure)
>         1
>         electrical 1
>         temperature 1
>       subsystems 1, 2

>     ### T

>       TCP/IP connections 1, 2
>         10Base-T 1
>         10Base-T Ethernet card 1
>         additional resources 1
>         Ethernet cables 1
>         Ethernet hub 1
>         IP addresses 1, 2
>         steps 1
>       Tool Kit 1
>         AC adapter 1
>         DC power supply 1
>         Demonstartion Board 1
>         plastic enclosure 1
>         programming cable 1
>         User's Manual 1
>         wire assembly 1

>     ### V

>       Vcc
>         J9-12 1

Z-World http://www.zworld.com Voice: (530) 757-3737 FAX: (530) 753-5141 sales@zworld.com