Rabbit 2000™ Microprocessor Benchmarks
The following table indicates the outstanding floating-point capability of the Rabbit 2000 microprocessor as compared to other processors. The Rabbit 2000's powerful number crunching ability and highly optimized Dynamic C software libraries provide superior floating-point performance.

Floating-Point Operation | RABBIT 2000 @ 29.49 MHz | Zilog Z180 @ 24.58 MHz | Dallas DS80C320 @ 33.18 MHz | Phillips 80C51 @ 33.18 MHz | AMD 188ES @ 36.86 MHz
Add | 9.6 µs | 26 | 32 | 78 | 194
Multipy | 12 µs | 42 | 34 | 85 | 184
Square Root | 32 µs | 343 | 334 | 805 | 355
Sine | 94 µs | 1238 | 452 | 1112 | 804

For details on the benchmarks tests and the C code used, view the following files.
The complete description of our bechmark tests / speedtest.pdf
The five C applications used to generate the benchmark results / bsource.zip